Check 1+1 MKSP Redundancy Status

May 200

Introduction

When using 1+1 Stream Processors (and for this example I am using 1+1 SP in Compact Mode). The 1+1 SP servers
There are several operations that the SPs are handling, and either SP can be the one doing an operation, these are:

StatMux
PSI
Scrambling CA
MUX

I am unsure of how tightly coupled these components are, i.e. do Mux and PSI always follow each other, I am unsure. StatMux and CA do seem to be quite independent though.
Please note - You must you the Management VIP for the IP Address for this to work.
In a web browser, enter the following:

http://your_MKSP_VIP_address:8080/api/mfsp/activeStandby/status?version=11.3