Check 1+1 MKSP Redundancy Status

May 200

Introduction

When using 1+1 Stream Processors (and for this example I am using 1+1 SP in Compact Mode). The 1+1 SP servers
There are several operations that the SPs are handling, and either SP can be the one doing an operation, these are:

StatMux
PSI
Scrambling CA
MUX

I am unsure of how tightly coupled these components are, i.e. do Mux and PSI always follow each other, I am unsure. StatMux and CA do seem to be quite independent though.
Please note - You must you the Management VIP for the IP Address for this to work.
In a web browser, enter the following:

http://your_MKSP_VIP_address:8080/api/mfsp/activeStandby/status?version=11.3

You will see an output in your browser similar to below (with different instance names) - If your output is one long line or lines of text, then install a JSON viewer plugin in to your browser.

{
mongo_status: "ok",
rabbit_status: "ok",
statmux: {
active: {
SP01: [
"MK01"
],
SP02: [ ]
},
inactive: {
SP01: [ ],
SP02: [
"MK01"
]
}
},
psi: {
active: {
SP01: [
"mux.mux_52_1_1.outputs.TS1"
],
SP02: [ ]
},
inactive: {
SP01: [ ],
SP02: [
"mux.mux_52_1_1.outputs.TS1"
]
}
},
mux: {
active: {
SP01: [
"mux_52_1_1"
],
SP02: [ ]
},
inactive: {
SP01: [ ],
SP02: [
"mux_52_1_1"
]
}
},
simulcrypt: {
active: {
SP01: [
"mux_52_1_1"
],
SP02: [ ]
},
inactive: {
SP01: [ ],
SP02: [
"mux_52_1_1"
]
}
}
}