UHD HD Switch

Jun 2021

Introduction

At the time of writing, the CE1 only operates in either HD or UHD mode (variant 1 and variant 2, don't ask me what variant 3 is).
So if the unit is set to UHD mode, you cannot do a HD encode (white lie, you can but the M1 CPU tries to upscale HD to UHD and you run out of CPU).
So to change mode you have to edit a file and then reboot the unit. This should be addressed around August 2021.

The Web UI for operation changes
The OS for Network Changes and Upgrades