Interface Config

Jan 2020

Introduction
When using the M1 chassis, it should have been installed using the official .ISO, so this is applicable to both RX1 and MKSP installation.
Even though the interface configuration may look okay, there is an issue with the way the interfaces are installed, to remedy this you can run a small script that will recreate all of the configuration files.
The script update_network_devices.sh can be downloaded here: