Reboot Command

July 2021

Introduction

The RX1 runs (at this time) on CentOS, and there are a couple of ways you can reboot the unit. From the command line you can issue the reboot command, or from the UI you can use the reboot button. There is a script however that can be used to reboot the unit, and this does a complete shutdown, and start up of the unit, the same as if the unit had been powered off, then on again.

Reboot Script

The reboot script is called rx1_power_cycle.sh and lives in the /opt/ericsson/mfcp/ location.
To use the script, from the command line simply enter the following:

sudo /opt/ericsson/mfcp/rx1_power_cycle.sh