RX9004 Rear Panel

Feb 2017

The RX9004 Rear panel is shown below.

S1 is generally what we use for ASI Inputs.

LAN1/LAN2 are for control (but can be used for data)

LAN3/LAN4 are generally for data input.

BNC1/BNC2/BNC3/BNC4 are for the SDI UHD Inputs and will work with quarter HD (QUAD) or 2SI feeds.