G6 2U Node Distribution

Platform model:Multi Screen Encoder
Serial number:4e-000064
Part number:IB-00035-01-XS
Firmware:Muse
Version:5.0.830 (021)
ISO version:MUSE-CUSTOM
Upgrade expiration: Unknown
Date:2016-08-17 11:44:56 +01:00
When using the G6 2U four node MFLE (Muse Live) you must explicitly designate one of the four nodes for each encoding profile, because by default they will all try to use the first node.
When createing a profile, on the Video Streams Settings page look for the section entitled Encoding Distribution