CE1

Jun 2021

Contribution Encoder

{{:t1_chassis.jpg?500|

The CE1 is the replacement for the AVP HEVC. It is M1 based like the RX1/MKSP but has some different hardware to allow it to perform encoding. The Main difference is the VEGA (Mellanox) card that can do (at this time) up to 4 HD encodes or 1 x UHD Encode. The CE1 supports HEVC and H264 at resolutions up to 2160p50 4:2:2 10 bit.

Login Details

Setting Interfaces

Interface Config

Check Bundle

HD UHD Switch

Delete Licenses

Check Mellanox Rivermax Card Serial

Manually Upgrade the Software Bundle on CE1