Connect to Server via MGMT Port

Oct 2017

Once a valid IP address has been assigned to the MGMT Port, shown below:
Then we can connect to the Management UI of the switch

http://ipaddress/shell/

MSH8900 login:

console admin

Please enter the Node number [1-9] or Switch [S]:

1

Selected node 1. Please enter payload number [1-2]:

1 selected Payload 1.

Using HPM.2 Draft extension for SOL Info: 2 SOL instances available

Info: SOL payload already de-activated Using HPM.2 Draft extension for SOL Info: 2 SOL instances available

[SOL Session operational. Use ~? for help]

** Console dropped due to BP Com request *

(you may have to enter login details of installed OS)

Press enter

You now have command prompt