G8 Interfaces

Oct 2019

The G8 has a few interface options, some of which are shown here. The units we have differ in the fact that on the right hand side, they have 4 x Gbe interfaces, not 2 x as shown here.
The demo units all are the 1074 style, and have the 5 spigot UHD Deltacast card fitted (not shown here).
The 2074 is a 2U unit that takes up to 4 x cartridge style servers. Due to their size, these servers are unable to take any PCI-E cards, so in a 2074 Transcode is the only option. (Ignoring the upcoming 20226-6 SDI over IP)